V1.1.0.0 STD Update Notes (compared with V1.0.0.0 STD)

**New features:**

1. Output capacity up to 10.4 million pixels
2. Image mosaic
3. Web control
4. Frame rate adjustment to AUX and MVR outputs
5. HDCP on and off

**Bug fixes:**

1. Fixed the problem that the brightness of grid lines under low grayscale is not uniform.
2. Fixed the problem that the conversion from RGB Limited to RGB Full for SDI input source does not take effect.
3. Fixed the problem that there are lines scrumbled at the bottom of the image for the SDI input source after it is scaled.

**Improvements:**

1. Optimized the aspect ratio of the software UI.
2. Optimized the interaction design for the TFT screen
3. Optimized the interaction design for the software.
4. Optimized the OSD text function.
5. Optimized the maximum number of OSD files that can be added from 16 to 8.
6. Improved the efficiency of BKG loading, preset loading, and preset switching.