**Firmware Program Release Notes**

# Basic Information

|  |  |
| --- | --- |
| Program Type (General or Customized) | General |
| Applicable Receiving Card | A8s |

# Chip List

|  |  |  |  |
| --- | --- | --- | --- |
| Program Package | Driver IC | Decoding Chip | Note |
| DATA\_A8s\_V4.7.2.0 | *MBI series: MBI5041(B), MBI5042(B), MBI5043, MBI515x, MBI5252, MBI5353;**SUM series: SUM2028, SUM203x, SUM213x;**MY series: MY9266, MY9269, MY9366;**ICN series: ICN2053;**SM series: SM16158, SM16159;**Others: TLC5958, TLC59581, SCL8060;* | *74HC138,**74HC595,**RT5953, RT5958,**SM5266, ICN2013,**ICN2018/2019* |  |
| DATA\_A8s\_V4.7.2.3 | *MBI series: MBI5251;* | *74HC138,**74HC595,**RT5953, RT5958,**SM5266, ICN2013,**ICN2018/2019* |  |

# Features

| Supported Features | Note |
| --- | --- |
| Maximum load capacity: 384×512 pixels (PWM IC); 384×384 (Common IC/LS99xx) | For module design, it is necessary to use horizontal conventional layout. Irregular layouts, such as column scanning, folding, or skipping pixels, may affect the maximum load. |
| Up to 1/64 scan |  |
| Up to 32 groups of parallel data; 64 groups of serial data (expandable to 128 groups of serial data) |  |
| Image booster (22bit+, precise grayscale) | NovaLCT5.4.0 and later |
| Color management |  |
| Pixel level brightness and chroma calibration |  |
| Quick seam correction |  |
| Low latency |  |
| 3D function | The load capacity will be halved when this function is enabled. |
| Individual gamma adjustment for RGB |  |
| 90° image rotation |  |
| Free image rotation |  |
| HDR function | The load capacity will be reduced by half for 10bit / 12bit video sources |
| Display of 3-color 1-point serial input and 3-color 16-point serial input |  |
| Smart module | Dedicated firmware required |
| Automatic module calibration |  |
| Stable uploading of calibration coefficients | Calibration acceleration supported |
| Quick uploading of calibration coefficients |  |
| Module Flash management |  |
| One click to apply calibration coefficients in module Flash |  |
| Mapping1.1 function |  |
| Settings of a stored image in the receiving card |  |
| Temperature & voltage monitoring |  |
| Cabinet LCD | Only 5-Pin LCD is supported |
| Bite error detection |  |
| Status detection of dual power supplies |  |
| Firmware program readback |  |
| Configuration parameter readback |  |
| Dual card backup and status monitoring |  |
| Loop backup |  |
| Dual backup of configuration parameters |  |
| Dual program backup |  |
| Dual backup of calibration coefficients |  |
| 10bit/12bit input source | The load capacity will be halved. |

# V4.7.2.0 Updates

|  |
| --- |
| New Features |
| * Supports the MBI5251 custom chip; Must work with NovaLCT V5.4.7.
 |
| Improvements |
| * None
 |
| Bug Fixes |
| * None
 |

# Others

|  |
| --- |
| 1. Must work with NovaLCT V5.4.7 or later. |